Fix these in a reprint run down the line.

* No silkscreen for SPI debug pins.
* LC circuit is wrong, need to use instrumentation amplifier for good performance.
* PT powered off of unregulated 12V supply. Need to use 10V or else we’re fucked.
* Burned out 5V LED, use bigger resistor next time.
* Should also take some time to make an ignition measurement device.